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EPSILON TB30
[bookmark: _GoBack]The Epsilon is a tandem seat, retractable tri‑gear, western technology production aircraft manufactured by Groupe Aerospatiale in France, w/Parts support by Daher
Max Level Speed	202 kts.	Engine ‑ 300 HP Lycoming AEI0 540L1B5D
VNE	281 kts.	Propeller‑Hartzell constant speed 78"
Stall speed	63 kts.	Gross Weight 2,755 Ibs.
G Limits	+ 6.75G/‑3.35G	Empty Weight 1,992 Ibs.
	Inverted Flight Duration 2 minutes	Fuel (useable) 55.4 gallons
Wing span 26'	Length 24.9'	Height 8.6'
S/N 38   N638TB  Mfg. 1985
Epsilon TB-30 Inc.
(805) 594‑0726
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